X509_REQ_PRINT_EX(3)

NAME
X509_REQ_print_ex, X509_REQ_print, X509_REQ_print_fp - pretty-print a PKCS#10 certification request

SYNOPSIS
int
X509_REQ_print_ex(BIO *bio, X509_REQ *req, unsigned long nameflags, unsigned long skipflags);
int
X509_REQ_print(BIO *bio, X509_REQ *req);
int
X509_REQ_print_fp(FILE *fp, X509_REQ *req);

DESCRIPTION
X509_REQ_print_ex() prints information contained in req to bio in human-readable form. Printing is aborted as soon as any operation fails, with the exception that failures while attempting to decode or print the public key are not considered as errors.

By default, the following blocks of information are printed in the following order. Each block can be skipped by setting the corresponding bit in skipflags, provided in parentheses after each block description.

•   A pair of lines reading "Certificate Request:" and "Data:" containing no information. (X509_FLAG_NO_HEADER)

•   The value contained in the version field in decimal and hexadecimal notation. (X509_FLAG_NO_VERSION)

•   The subject name is printed with X509_NAME_print_ex(3). (X509_FLAG_NO_SUBJECT)

•   The public key algorithm is printed with i2a_ASN1_OBJECT(3), and the public key returned from X509_REQ_get_pubkey(3) with EVP_PKEY_print_public(3). (X509_FLAG_NO_PUBKEY)

•   For each X.501 attribute that is not a requested extension according to X509_REQ_extension_nid(3), the object identifier is printed with i2a_ASN1_OBJECT(3), and all values of the types V_ASN1_PRINTABLESTRING, V_ASN1_T61STRING, and V_ASN1_IA5STRING are printed with BIO_write(3). (X509_FLAG_NO_ATTRIBUTES)

•   The requested extensions are retrieved with X509_REQ_get_extensions(3) and their types and values are printed with i2a_ASN1_OBJECT(3) and X509V3_EXT_print(3), or, if the latter fails, with ASN1_STRING_print(3). (X509_FLAG_NO_EXTENSIONS)

•   The signature is printed with X509_signature_print(3). (X509_FLAG_NO_SIGDUMP)

The nameflags argument modifies the format for printing X.501 Name objects contained in req. It is passed through to X509_NAME_print_ex(3). If nameflags is X509_FLAG_COMPAT, the indent argument of X509_NAME_print_ex(3) is set to 16 spaces and the traditional SSLeay format generated by X509_NAME_print(3) is used. Otherwise, if the only bit set in XN_FLAG_SEP_MASK is XN_FLAG_SEP_MULTILINE, indent is set to 12 spaces. Otherwise, indent is set to zero.

X509_REQ_print() is a wrapper function setting the nameflags to XN_FLAG_COMPAT and the skipflags to X509_FLAG_COMPAT.

X509_REQ_print_fp() is similar to X509_REQ_print() except that it prints to fp.

RETURN VALUES
These functions return 1 if all requested information was successfully printed, even if failures occurred while attempting to decode or print the public key, or 0 if any operation fails.

SEE ALSO
BIO_new(3), X509_print_ex(3), X509_REQ_new(3)

HISTORY
X509_REQ_print() first appeared in SSLeay 0.4.4 and X509_REQ_print_fp() in SSLeay 0.6.0. These functions have been available since OpenBSD 2.4.

X509_REQ_print_ex() first appeared in OpenSSL 0.9.7 and has been available since OpenBSD 3.2.

BUGS
Some printing failures are silently ignored while printing extensions, which may result in incomplete data being printed.